**Guidance Note No: 35/99 Revision No: 10**

**This Guidance Notice only applies to vessels that were operating commercially on 30 June 2013**

# Fishing vessels (class 3C and 3B) less than 8 metres in measured length operating outside declared sheltered waters limits

**Requirements for Safety Equipment and Operator Qualifications   
Class 3C (within 30 nautical miles of the coastline) and   
3B (within 200 nautical miles of the coastline)**

**Fishing Tour Operators are Class 2 vessels and are not covered by this Guidance Note.**

Under the NT Marine Act, fishing vessels (Class 3C and 3B) less than 8 metres in length operating subject to the NT Marine Act are **exempt** from **survey** but must carry safety equipment as required by the Marine (Safety) Regulations and be operated by persons holding qualifications as required by the NT Marine (Safety Manning) Regulations.

**Note: For fishing vessels less than 6.2 metres operating within 5 nautical miles of the coast or a mother ship refer to GN No. 60/2001 and GN No. 61/2001.**

Gazetted sheltered waters are detailed in Guidance Note No 33/98.

Minimum Safety Manning requirements for fishing vessels are specified in Guidance Note No. 28/96

Radio requirements are detailed in Guidance Note No: 91/2002.

Details of prescribed safety equipment are as follows:

|  |
| --- |
| **Barometer**  Barometer or barograph |
| **Bilge alarm**  One to be fitted in any space containing inboard propelling machinery. (Not required on vessels powered by outboard motors). |
| **Bilge pumps**  One manual bilge pump with a capacity of not less than 4.0 Kl/hr. Note: A power driven bilge pump of the same capacity may be substituted. |
| **Charts and nautical publications**  To be suitable for the area of operation |
| **Clock**  Clock or wristwatch |
| **Code flags**  Flags "N" and "C" |
| **Compass**  Magnetic Steering Compass placed in a suitable position for taking accurate observations Note: A compass is required to be swung every 4 years and a copy of the deviation card must be kept on board the vessel. |
| **Depth sounding device**  Mechanical depth sounding device or hand lead line |
| **Distress signals**  Three parachute distress rockets Two red hand flares One hand held orange smoke signal  Note: Expiry date of flares must be valid. |
| **Electric installation/equipment – emergency**  Two waterproof torches, one of which must be a signalling torch. |
| **Emergency Position Indicating Radio Beacon (EPIRB)**  ***Class 3C***  406MHz EPIRB to AS/NZS 4280 requirements.  ***Class 3B***  406MHz EPIRB to AS/NZS 4280 requirements  Note: Expiry date of battery must be valid. |
| **Fire buckets**  One with lanyard of sufficient length to allow the bucket to be easily filled over the side of the vessel. |
| **Fire extinguishers – portable**  One suitable for extinguishing oil fires for use in each space containing propelling machinery with a minimum rating of 30B.  Note: Portable extinguishers must be serviced every 12 months. |
| **Gas detector**  For LPG installations a gas detector shall be fitted with sensors as close as possible to the source of entry below deck. |
| **Lifebboats & liferafts**  ***Class 3B***  Coastal liferaft(s) for 100% complement.  ***Class 3C***  Coastal Liferaft(s) for 100% complement or; Dinghy for 100% complement (This option is not allowed after 1st December 2012) or: Internal buoyancy as prescribed in Section 10 of the USL Code. |
| **Lifebuoys**  1 lifebuoy with light (this is not required for a vessel which carries only one (1) person). |
| **Lifejackets**  ***Class 3B***  A SOLAS Lifejacket with light and whistle for each person. Note: Expiry date of lifejacket light must be valid.  ***Class 3C***  A COASTAL lifejacket with light and whistle for each person. Note: Expiry date of lifejacket light must be valid. |
| **Medicines and medical stores**  ***Class 3B***  As per both Scale E and Scale F  ***Class 3C***  As per Scale F  See appendix |
| **Navigation lights and shapes**  Lights: Port, starboard, masthead, stern, anchor and fishing or trawling lights.  Note: A power driven vessel of less than 12 metres may exhibit an all round white light in lieu of masthead and stern lights and this can also serve as an anchor light.  Day Shapes: Basket |
| **Sound signal**  Some means of making an efficient sound signal. Such as a portable air or gas operated horn. |
| **Anchors and cables**  Anchors and cables - sufficient in number, weight and strength, as detailed in Section 13 of the USL Code.  Hawsers and warps of sufficient number, weight and strength having regard to the size and service of the vessel. |
| **Radiotelephony**  Single side band installation.  Note: You must contact any one of the following companies listed in Guidance Note: 91/2002 to ensure radio is satisfactory. |

For further information please contact this office.

Signed by: Sri Srinivas, Principal Marine Surveyor  
Date Issued: 28 November 2011

| **For further information contact Marine Safety Branch:** |
| --- |
| 2nd Floor, Energy House, 18-20 Cavenagh, Darwin NT 0800, GPO Box 2520, Darwin NT 0801 |
| Telephone: 08 8924 7100, Facsimile: 08 8924 7009 |
| Email: [marinesafety@nt.gov.au](mailto:marinesafety@nt.gov.au) |

**Disclaimer:** While care is taken to ensure that information contained in NT Government publications is true and correct at the time of the publication, this information is provided on the basis that users undertake responsibility for assessing the relevance, accuracy and currency of its content. The Northern Territory of Australia gives no warranty or assurance and makes no representation, express or implied, as to the accuracy of this information or that it is suitable for your intended use. To the maximum extent permitted by law, each user waives and releases the Territory from any and all claims relating to the use of this information and in no event shall the Territory of Australia be liable for loss or damage arising directly or indirectly from the use of or reliance on it for whatever purpose.

## Appendix – Medicines and medical stores – Scale E

**Legend**

\* = Requires prescription

# = Requires separate locked storage and recording in controlled drug register

| **Description** | **Quantity** | **Expiry dated** | **Comments** |
| --- | --- | --- | --- |
| Antibiotic ointment 15g or 20g | 1 | Yes \* | infected wound |
| Chloramphenicol Eye Ointment 4g | 1 | Yes \* | eye antibiotic |
| Glyceryl trinitrate 400mcg spray | 1 | Yes | angina/ heart pain |
| Paracetamol 500mg/Codeine 30mg tabs | 20 | Yes \* | moderate-severe pain also cough suppression |
| Prochlorperazine 5mg tablet | 25 | Yes \* | nausea, giddiness |
| Prochlorperazine 25mg suppositories | 5 | Yes \* | vomiting, giddiness |
| Salbutamol inhaler | 1 | Yes | asthma attack |
| Sodium chloride and glucose or dextrose | 10 | Yes | rehydration |
| compound, powder sachets, 4.9g approx |  |  |  |
| Scalpel, sterile, disposable | 3 |  |  |
| Splint set, vacuum or air inflation | 1 |  |  |
| Neck collar, multi-size, rigid, fully adjustable | 1 |  |  |
| BVM air resuscitator | 1 |  |  |

## Appendix – Medicines and medical stores – Scale F

| **Article** | **Quantity** | **Expiry dated** | **Comments** |
| --- | --- | --- | --- |
| Bandage, conforming 5 cm | 2 |  | secure dressing and support injured parts |
| Bandage, conforming 10 cm | 2 |  | secure dressing and support injured parts |
| Bandage, heavy crepe 7.5 cm | 2 |  | support bandage |
| Bandage, heavy crepe 10 cm | 1 |  | support bandage, wide |
| Bandage, triangular | 4 |  | sling |
| Dressing, combine 10 x 10 cm, sterile | 3 | Yes | bleeding control |
| Dressing, combine 10 x 20 cm, sterile | 5 | Yes | bleeding control, large |
| Dressing, non-adherent (10 x 10 cm or similar) | 10 | Yes | wound cover |
| Dressing, hydroactive (10 x 10 cm or similar) | 2 | Yes | blisters, burns and minor |
| Wound dressing, combination, large | 3 |  | Major wounds |
| Wound dressing, combination, small | 2 |  | Major wounds |
| Adhesive roll non-woven fabric 5 cm x 10 m | 1 |  | securing dressings |
| Dressings, elastic fabric strips | 50 |  | minor wound cover |
| Gauze swabs, sterile (single use pkt of 3) | 9 | Yes | cleansing/dressing wound |
| Eye pad, sterile | 4 | Yes | eye cover |
| Wound closure strips, wide, 6 x 38 mm | 3 | Yes | securing wound sides |
| Tape surgical waterproof 2.5 cm x 5 m | 1 |  | Secure dressing |
| Tape surgical waterproof 5 cm x 5 m | 1 |  | Secure dressing |
| Towels, disposable, pkt of 2 | 3 |  |  |
| Plastic bag set (3 asst L, M and S) | 2 |  | Amputated parts |
| Plastic bag | 2 |  | disposal of soiled dressings |
| Gloves, disposable, large | 10 |  |  |
| Safety pins, stainless, assorted pkt of 12 | 1 |  |  |
| Blanket, emergency thermal | 1 |  | Hypothermia and shock |
| Ice pack, instant | 1 |  |  |
| Resuscitation mask, disposable | 1 |  |  |
| Resuscitation mask, pocket | 1 |  |  |
| Splinter probes, sterile, disposable | 10 |  |  |
| Splinter forceps, 12.5 cm | 1 |  |  |
| Shears, stainless, 19 cm minimum | 1 |  |  |
| Scalpel, disposable | 2 |  |  |
| Splint malleable, universal | 2 |  |  |
| Normal saline, sterile 30 ml polyamp | 10 | Yes | eye irrigation / wound |
| Povidone iodine swabs (single use) | 20 | Yes | Antiseptic |
| Anaesthetic + antiseptic cream 30 g | 1 | Yes |  |
| Hydrocortisone 1% cream 30 g | 1 | Yes | rashes & bites |
| Paracetamol 500 mg tabs or caps | 2 x 24 | Yes | mild pain relief |
| Paracetamol 500 mg / Codeine 8 mg | 24 | Yes | moderate pain relief |
| Ibuprofen 200 mg tablets | 24 | Yes | anti-inflammatory |
| Hyoscine hydrobromide 0.3mg tablets | 10 | Yes | Seasickness |
| Loperimide 2mg tablets | 16 | Yes | diarrhoea |
| Loratadine HCl 10 mg or Fexofenadine HCl | 10 | Yes | antihistamine (non-sedating) |
| 120 mg tablets |  |  |  |
| Antacid tablets | 50 | Yes |  |
| CPR instruction chart or card | 1 |  |  |
| Australian First Aid Book | 1 |  |  |