**Guidance Note No: 60/01 Revision No: 6**

**This Guidance Notice only applies to vessels that were operating commercially on 30 June 2013**

# Requirements for survey and manning exempt fishing vessels (Class 3D, 3C and 3B)

* less than 6.2 Metres in Length Operating within 5 Nautical Miles of the Coast or
* operating with a Mother Vessel, all Vessels being within 5 Nautical Miles of the Coast)

Fishing Tour Operators are Class 2 vessels and are not covered by this Guidance Note.

In accordance with amendments to Sections 23 and 75 of the NT Marine Act which came into force on the 2nd April 2001:

“Fishing vessels less than 6.2 metres in length that are operating within a limit of 5 nautical miles of the coast” are not required to be in survey nor be operated by a coxswain, however, they are required to carry safety equipment as detailed below.

Under Sections 96 to 101; 109 to 115B and 117, the non-carriage of specified safety equipment and operating an unsafe vessel etc are offences and penalties apply.

|  |
| --- |
| **Bailer**One with lanyard of at least 4 litre capacity |
| **Bilge alarm**One to be fitted in any space containing inboard propelling machinery. (Not required on vessels powered by outboard motors.) |
| **Bilge pumps**One bilge pump of at least 4000 litres per hour capacity |
| **Charts and nautical publications**To be suitable for the area of operation of vessel [not required for vessels operating in conjunction with a mothership] |
| **Clock**Clock or wristwatch |
| **Code flags**Flags “N” and “C” |
| **Compass**At least one (1) hand held |
| **Depth sounding device**Mechanical depth sounding device or hand lead line |
| **Distress signals**Three parachute distress rocketsTwo red hand flaresOne hand held orange smoke signalNote: Expiry date of rockets and flares must be valid. |
| **Electric installation/equipment – emergency**At least one torch |
| **Emergency Position Indicating Radio Beacon (EPIRB)**One 406 MHz EPIRB to AS/NZS 4280 requirements.Note: Expiry date of battery must be valid for period of survey and must be registered with AUSSAR |
| **Fire extinguishers – portable**One suitable for extinguishing oil fires with a minimum rating of 30B. |
| **Gas detector**For LPG installations a gas detector shall be fitted with sensors as close as possible to the source of entry below deck. |
| **Life buoys**One life buoy with light |
| **Life jackets**One Coastal life jacket with light and whistle per person. |
| **Medicines and medical stores**Scale GSee appendix |
| **Navigation lights and shapes**A white light visible all round and separate or combined sidelights. The white all round light shall be carried at least 1 metre above the sidelights. Vessels with maximum speed not exceeding 7 knots need not exhibit separate or combined sidelights. |
| **Radiotelephony**VHF Walkie talkie suitable for search and rescue. |
| **Remote stops for other machinery**To be provided for oil fuel, lubricating oil and hydraulic oil pumps and also separators. |
| **Signalling light**A signalling light or suitable approved torch fitted with a flashing button in addition to an ON/OFF button. An ordinary torch is NOT acceptable. |
| **Sound signal**Portable sound signal. |
| **Windlass, anchors and cables**One Danforth or CQR Anchor of minimum 17 LBS attached to 3m of 8mm chain attached to 70 metres of 12 mm rope. Reef anchor if carried will be in addition to above. |
| **Operational and safety procedure handbooks**Operational and Safety procedure handbooks developed by operators /owners/ NTFIC in conjunction with appropriate individuals and organisations must be kept on board. |
| **Internal buoyancy**Minimum manufacturer’s standard internal buoyancy. If vessel is not a standard production model, the owner must fit buoyancy to Appendix N Section 10 of USL Code. |
| **Drinking water**At least 5 litres of freshwater per day per person must be carried. |
| **Watertight container**One watertight buoyant container for carrying small gear like flares, etc. |

Signed by: Sri Srinivas
Date Issued: 28 July 2011

| **For further information contact Marine Safety Branch:** |
| --- |
| 2nd Floor, Energy House, 18-20 Cavenagh, Darwin NT 0800, GPO Box 2520, Darwin NT 0801 |
| Telephone: 08 8924 7100, Facsimile: 08 8924 7009 |
| Email: marinesafety@nt.gov.au |

**Disclaimer:** While care is taken to ensure that information contained in NT Government publications is true and correct at the time of the publication, this information is provided on the basis that users undertake responsibility for assessing the relevance, accuracy and currency of its content. The Northern Territory of Australia gives no warranty or assurance and makes no representation, express or implied, as to the accuracy of this information or that it is suitable for your intended use. To the maximum extent permitted by law, each user waives and releases the Territory from any and all claims relating to the use of this information and in no event shall the Territory of Australia be liable for loss or damage arising directly or indirectly from the use of or reliance on it for whatever purpose.

## Appendix

### Medicines and medical stores – Scale G

| **Description** | **Quantity** | **Expiry dated** | **Comments** |
| --- | --- | --- | --- |
| Bandage, conforming 5 cm | 1 |  | secure dressing and support |
| Bandage, conforming 10 cm | 1 |  | secure dressing and support |
| Bandage, heavy crepe 7.5 cm | 2 |  | support bandage |
| Bandage, triangular | 4 |  | sling |
| Dressing, combine 10 x 10 cm, sterile | 3 | Yes | bleeding control |
| Dressing, combine 10 x 20 cm, sterile | 2 | Yes | bleeding control, large |
| Dressing, non-adherent (10 x 10 cm or similar) | 5 | Yes | wound cover |
| Dressing, hydroactive (10 x 10 cm or similar) | 1 | Yes | blisters, burns and minor |
| Wound dressing, combination, large | 2 |  | Major wounds |
| Wound dressing, combination, small | 2 |  | Major wounds |
| Adhesive roll non-woven fabric 5 cm x 10 m | 1 |  | securing dressings |
| Dressings, elastic fabric strips | 50 |  | minor wound cover |
| Gauze swabs, sterile (single use pkt of 3) | 3 | Yes | cleansing/dressing wound |
| Eye pad, sterile | 2 | Yes | eye cover |
| Wound closure strips, wide, 6 x 38 mm | 1 | Yes | securing wound sides |
| Tape surgical waterproof 2.5 cm x 5 m | 1 |  | Secure dressing |
| Tape surgical waterproof 5 cm x 5 m | 1 |  | Secure dressing |
| Towels, disposable, pkt of 2 | 2 |  |  |
| Plastic bag set (3 asst L, M and S) | 1 |  | Amputated parts |
| Plastic bag | 2 |  | disposal of soiled dressings |
| Gloves, disposable, large | 10 |  |  |
| Safety pins, stainless, assorted pkt of 12 | 1 |  |  |
| Blanket, emergency thermal | 1 |  | Hypothermia and shock |
| Ice pack, instant | 1 |  |  |
| Resuscitation mask, disposable | 1 |  |  |
| Splinter probes, sterile, disposable | 5 |  |  |
| Splinter forceps, 12.5 cm | 1 |  |  |
| Shears, stainless, 19 cm minimum | 1 |  |  |
| Splint malleable, universal | 1 |  |  |
| Normal saline, sterile 30 ml polyamp | 6 | Yes | eye irrigation / wound cleaning |
| Povidone iodine swabs (single use) | 10 | Yes | Antiseptic |
| Anaesthetic + antiseptic cream 30 g | 1 | Yes |  |
| Paracetamol 500 mg tabs or caps | 24 | Yes | mild pain relief |
| Hyoscine hydrobromide 0.3mg tablets | 10 | Yes | Seasickness |
| Loperimide 2mg tablets | 16 | Yes | diarrhoea |
| Antacid tablets | 12 | Yes |  |
| CPR instruction chart or card | 1 |  |  |
| Australian First Aid Book | 1 |  |  |